|  |  |
| --- | --- |
|  |  |

**Product Guide Specification**

Specifier Notes: This product guide specification is written according to the Construction Specifications Institute (CSI) 3-Part Format, based on *MasterFormat 2016* and *The Project Resource Manual—CSI Manual of Practice. The Manufacturer is responsible for technical accuracy.*

The section must be carefully reviewed and edited by the Architect or Engineer to meet the requirements of the project and local building code. Words and sentences within brackets [ ] are choices to include or exclude a particular item or statement. Coordinate this section with other specification sections and the Drawings. Delete all “Specifier Notes” after editing this section.

**Section 28 21 00: Video Surveillance**

**Section 28 21 13: IP Cameras**

**IP CAMERA**

1. **– GENERAL** 
   1. SUMMARY
      1. Section Includes
         1. Section 28 21 17: Video Surveillance – Surveillance Cameras – Camera Housings
         2. Section 28 21 19: Video Surveillance – Surveillance Cameras – Camera Mounts
         3. Section 28 27 00: Video Surveillance – Video Surveillance Sensors
      2. Related Sections
         1. [Section 28 33 15: Security Detection, Alarm and Monitoring – Security Monitoring and Control – Security Monitoring and Control Software].

\*\*\*\*\*\*\*\*\*\* Specifier’s note: Include those standards referenced elsewhere in this SECTION.

* 1. REFERENCES

|  |  |
| --- | --- |
| STANDARD | CE-LVD: EN62368-1; CE-EMC: Electromagnetic Compatibility Directive 2014/30/EU; CE-RED: Radio Equipment Directive 2014/53/EU; FCC: 47 CFR FCC Part 15, Subpart B; FCC ID: FCC PART 15C; |

* 1. SYSTEM DESCRIPTION
     1. Section Includes
        1. Video Surveillance – Surveillance Cameras –IP CAMERA
  2. SUBMITTALS
     1. Product Data:
        1. Manufacturer’s data, user and installation manuals for all equipment and software programs including computer equipment and other equipment required for complete video management system.
     2. Dimensional Drawings; include
        1. Overall device dimensions.
        2. Dimensions specific for installation.
     3. Closeout Submittals
        1. User manual.
        2. Parts list.
        3. Maintenance requirements.
  3. QUALITY ASSURANCE
     1. Manufacturer:
        1. Minimum of [10] years of experience in manufacture and design Video Surveillance Devices.
     2. Video Surveillance System:
        1. List certifying bodies (UL, etc.)
        2. Provide evidence of compliance upon request.
     3. Installer:
        1. Minimum of [5] years of experience installing Video Surveillance System.
  4. DELIVERY, STORAGE AND HANDLING
     1. Comply with requirements of Section 01 60 00.
     2. Deliver materials in manufacture’s original, unopened, undamaged containers; and unharmed original identification labels.
     3. Protect store materials from environmental and temperature conditions following manufacturer’s instructions.
     4. Handle and operate products and systems according to manufacturer’s instructions.
  5. WARRANTY
     1. Provide manufacturer’s warranty covering [3] years for replacement and repair of defective equipment. Warranty varies country to country.
  6. MAINTENANCE
     1. Make ordering of new equipment for expansions, replacements, and spare parts available to dealers and end users.
     2. Provide factory direct technical support via phone and e-mail.

1. **– PRODUCTS**
   1. MANUFACTURERS
      1. Acceptable Manufacturer:

ZHEJIANG DAHUA VISION TECHNOLOGY CO., LTD.

Address: No.1399, Binxing Road, Binjiang District, Hangzhou, P.R. China

Postcode: 310053

Tel: +86-571-87688888 28933188

Email: dhoverseas@dhvisiontech.com

Website: www.dahuasecurity.com

* + 1. Substitutions:
       1. [All proposed substitutions must be approved by the Architect or Engineer professional.]
       2. [Proposed substitutions must provide a line-by-line compliance documentation.]
  1. IP CAMERA | DH-IPC-HDBW1430DEN-SW-0280B

|  |  |  |
| --- | --- | --- |
| Camera | Image Sensor | 1/3" CMOS |
| Camera | Max. Resolution | 2560 (H) × 1440 (V) |
| Camera | ROM | 16 MB |
| Camera | RAM | 64 MB |
| Camera | Scanning System | Progressive |
| Camera | Electronic Shutter Speed | Auto/Manual 1/3 s–1/100,000 s |
| Camera | Min. Illumination | 0.03 lux@F2.0 (Color, 30 IRE); 0.003 lux@F2.0 (B/W, 30 IRE); 0 lux (Illuminator on) |
| Camera | S/N Ratio | ＞56 dB |
| Camera | Illumination Distance | Up to 30 m (98.43 ft) (IR LED) |
| Camera | Illuminator On/Off Control | Auto; Manual |
| Camera | Illuminator Number | 3 (IR LED) |
| Camera | Angle Adjustment | Pan: 0°–355°; Tilt: 0°–75°; Rotation: 0°–355° |
| Lens | Lens Type | Fixed-focal |
| Lens | Lens Mount | M12 |
| Lens | Focal Length | 2.8 mm |
| Lens | Max. Aperture | F2.0 |
| Lens | Field of View | H: 90°; V: 50°; D: 107° |
| Lens | Iris Control | Fixed |
| Lens | Close Focus Distance | 1.0 m (3.28 ft) |
| Lens | DORI Distance | D: 68 m; O: 27.2 m; R: 13.6 m; I: 6.8 m (D: 223.10 ft; O: 89.24 ft; R: 44.62 ft; I: 22.31 ft) |
| Video | Video Compression | H.264B; H.264; H.264H; H.265 |
| Video | Smart Codec | Smart H.265+; Smart H.264+ |
| Video | Video Frame Rate | Main stream: 2560 × 1440@(1–20 fps) Sub stream: 640 × 480@(1–25/30 fps) \*The values above are the max. frame rates of each stream; for multiple streams, the values will be subjected to the total encoding capacity. |
| Video | Streaming Capability | 2 streams |
| Video | Resolution | 4M (2560 × 1440); 3M (2304 × 1296); 1080p (1920 × 1080); 1.3M (1280 × 960); 720p (1280 × 720) |
| Video | Bit Rate Control | CBR/VBR |
| Video | Video Bit Rate | H264: 24 kbps–4096 kbps H265: 9 kbps–4096 kbps |
| Video | Day/Night | Auto(ICR)/Color/B/W |
| Video | BLC | Yes |
| Video | WDR | DWDR |
| Video | White Balance | Auto; natural; street lamp; outdoor; manual; regional custom |
| Video | Gain Control | Auto |
| Video | Noise Reduction | 3D NR |
| Video | Motion Detection | OFF/ON (4 areas, rectangular) |
| Video | Region of Interest (RoI) | Yes (4 areas) |
| Video | Smart Illumination | Yes |
| Video | Image Rotation | 0°/180° |
| Video | Mirror | Yes |
| Alarm | Alarm Event | No SD card; SD card full; SD card error; network disconnection; IP conflict; illegal access; motion detection; video tampering |
| Network | Network Port | RJ-45 (10/100 Base-T) |
| Network | Wi-Fi | IEEE 802.11b/g/n 2.4000–2.4835 GHz, 2.4 G, EIRP≤20 dBm (CE), output power≤30 dBm (FCC) |
| Network | SDK and API | Yes |
| Network | Network Protocol | IPv4; HTTP; TCP; UDP; ARP; RTP; RTSP; RTCP; DHCP; DNS; NTP; Multicast;RTMP |
| Network | Interoperability | ONVIF (Profile S & Profile G); CGI; P2P |
| Network | User/Host | 6 (Total bandwidth: 36 M) |
| Network | Storage | Micro SD card (support max. 256 GB, sold separately) |
| Network | Browser | IE Chrome Firefox |
| Network | Management Software | Smart PSS;DSS;DMSS |
| Network | Mobile Client | iOS; Android |
| Network | Cyber Security | Video encryption; Configuration encryption; Digest; WSSE; Account lockout; Security logs; Generation and importing of X.509 certification; HTTPS; Trusted boot; Trusted execution; Trusted upgrade |
| Power | Power Supply | 12 VDC |
| Power | Power Consumption | Basic: 2 W (12 VDC); Max. (H.265+IR intensity): 4.9 W (12 VDC) |
| Environment | Operating Temperature | –40 °C to +60 ℃ (–40 °F to +140 °F) |
| Environment | Operating Humidity | ≤95% |
| Environment | Storage Temperature | –30 °C to +60 ℃ (–22 °F to +140 °F) |
| Environment | Protection | IP67; IK10 |
| Structure | Casing Material | Metal |
| Structure | Product Dimensions | Φ110.7 mm × 88.7 mm (Φ4.33" × 3.49") |
| Structure | Net Weight | 414 g (0.91 lb) |
| Structure | Gross Weight | 592 g (1.31 lb) |
| Structure | Installation | Wall mount; in-ceiling mount; pole mount (vertical) |

1. **– EXECUTION**
   1. EXAMINATION
      1. Examine areas to receive devices and notify adverse conditions affecting installation or subsequent operation.
      2. Do not begin installation until unacceptable conditions are corrected.
   2. PREPARATION
      1. Protect devices from damage during construction.
   3. INSTALLATION
      1. Install devices in accordance with manufacturer’s instruction at locations indicated on the floor drawings plans.
      2. Perform installation with qualified service personnel.
      3. Install devices in accordance with the National Electrical Code or applicable local codes.
      4. Ensure selected location is secure and offers protection from accidental damage.
      5. Location must provide reasonable temperature and humidity conditions, free from sources of electrical and electromagnetic interference.
   4. FIELD QUALITY CONTROL
      1. Test snugness of mounting screws of all installed equipment.
      2. Test proper operation of all video system devices.
      3. Determine and report all problems to the manufacturer’s customer service department.
   5. ADJUSTING
      1. Make proper adjustment to video system devices for correct operation in accordance with manufacturer’s instructions.
      2. Make any adjustment of camera settings to comply with specific customer’s need.
   6. DEMOSTRATION
      1. Demonstrate at final inspection that video management system and devices functions properly.

END OF SECTION